{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["الأبعاد","الوحدة","","الارتفاع","mm","550","550"]
["","","","العرض","mm","765","765"]
["","","","العمق","mm","285","285"]
["الوزن","الوحدة","","","kg","41","41"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","rpm","500","500"]
["","","التدفئة","منخفض جداً","rpm","500","500"]
["Compressor","Type","","","","ضاغط متأرجح محكم مانع للتسريب","ضاغط متأرجح محكم مانع للتسريب"]
["Sound pressure level","Cooling","","High","dBA","48","48"]
["","Heating","","High","dBA","50","50"]
["سائل تبريد","النوع","","","","R-32","R-32"]
["","السعة","","","kg","1.15","1.15"]
["","السعة","","","tCO2Eq","0.78","0.8"]
["","GWP","","","","675","675.0"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","م","15.0","15.0"]
["","","IU - IU","Max.","م","7.5","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","30","30"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","فولت","220-230-240","220-230-240"]
["Notes","","","","","(1) - لغرفة واحدة","(1) - يمكن تصميم كل نظام D-AHU احترافي بحسب احتياجاتك. حدد وحدة معالجة الهواء AHU التي تريدها على tools.daikinapplied.eu"]