{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 3MXM-N"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 3MXM40N2V1B","CTXM15M2V1B / CTXM15M2V1B / CTXM15M2V1B / 3MXM40N2V1B","CTXM15M2V1B / CTXM15M2V1B / 3MXM52N2V1B","CTXM15M2V1B / CTXM15M2V1B / CTXM15M2V1B / 3MXM52N2V1B","CTXM15M2V1B / CTXM15M2V1B / CTXM15M2V1B / 3MXM68N2V1B","CTXM15M2V1B / CTXM15M2V1B / 3MXM68N2V1B"]
["Cooling capacity","Nom.","","كيلوواط","3.00","4.00","3.00","4.50","4.50","3.00"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","293","386","274","450","302","252"]
["","نسبة فعالية استهلاك الطاقة","","","5.12","5.18","5.48","5.00","7.46","5.96"]
["","عامل الأداء","","","5.25","5.32","5.42","4.87","4.91","4.45"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","كيلوواط","3.60","4.60","3.60","6.80","6.50","5.30"]