{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["الدخل","النوع","","","","لوحة اللمس (مدخل تمثيلي مشفّر 10 بت)"]
["Ambient temperature","الرطوبة النسبية <","","","%","85"]
["","Operation","","Min.","درجة مئوية","0"]
["","","","Max.","درجة مئوية","40"]
["Maximum number of connectable indoor units","","","","","64, 128 (1)"]
["الاتصال","DIII-NET","","الكمية","","1"]
["","","","ملاحظة","","خط اتصالات أجهزة تكييف الهواء"]
["","‎10BASE-T","","ملاحظة","","خيار ويب"]
["","Ethernet","","ملاحظة","","منفذ للوصول إلى ويب ووظيفة البريد الإلكتروني"]
["","محطة الإدخال الطرفية","رقمي","الكمية","","1"]
["","","","ملاحظة","","إيقاف تشغيل إجباري"]
["","","نبضة","الكمية","","3"]
["","","","ملاحظة","","نبضة قياس الطاقة"]
["","المودم","","ملاحظة","","إمكانية توفر مودم على اللوحة"]
["","PCMCIA","","ملاحظة","","بطاقة ذاكرة فلاش"]
["","RS-232C","","ملاحظة","","محول DIII-NET plus"]
["Dimensions","Unit","","العرض","mm","230"]
["","","","العمق","mm","107"]
["","","","الارتفاع","mm","147"]
["شاشة LCD","النوع","","","","QVGA (320 x 240)‎‏، 4096 لوناً"]
["","الأبعاد","","العرض","inch","5.7"]
["الحد الأعلى لعدد الوحدات الخارجية القابلة للتوصيل","","","","","10, 20 (1)"]
["Power supply","Frequency","","","Hz","50/60"]
["","Voltage","","","V","100-240 (مزوّدة خارجياً)"]
["Notes","","","","","(1) - الترافق مع DCS601A51"]