{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZAG-B"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RZAG35B5V1B","FFA35A2VEB9 / RZAG35B5V1B","FFA60A2VEB9 / RZAG50B5V1B","FFA50A2VEB9 / RZAG50B5V1B","FFA60A2VEB9 / RZAG60B5V1B"]
["Cooling capacity","Min.","","كيلو واط","1.6","1.6","1.7","1.7","1.7"]
["","Nom.","","كيلو واط","3.5","3.5","5","5","6"]
["","Max.","","كيلو واط","4.5","4.5","6","6","6.5"]
["Heating capacity","Min.","","كيلو واط","1.4","1.4","1.5","1.5","1.6"]
["","Nom.","","كيلو واط","4","4","5.8","5.8","7"]
["","Max.","","كيلو واط","5","5","6","6","7.5"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.25","4","3.62","3.4","3.23"]
["","عامل الأداء","","","3.94","3.71","3.15","3.1","2.9"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","412","438","691","735","929"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A"]
["","","تدفئة","","A","A","D","D","D"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A+"]
["","الاستطاعة","Pdesign","كيلو واط","3.5","3.5","5","5","6"]
["","SEER","","","6.81","6.4","6.43","6.3","5.8"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","180","191","272","278","362"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+","A","A+","A+","A+"]
["","الاستطاعة","Pdesign","كيلو واط","4.2","4.2","4.3","4.3","4.5"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.04","3.8","4.08","4.01","4.04"]
["","Pdh استطاعة التدفئة عند -10°","","كيلو واط","3.53","3.5","3.68","3.66","3.87"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1455","1546","1474","1501","1558"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]