{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-L"]
[]
[]
[]
[]
["","","","","","RXN25LV1B","RXN35LV1B (Archived)","RXN50LV1B (Archived)","RXN60LV1B (Archived)"]
["Sound pressure level","Cooling","","High","dBA","","48","51","51"]
["Refrigerant","Charge","","","TCO2Eq","","2.1","3","3.1"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.00","1.45","1.50"]
["","النوع","","","","","R-410A","R-410A","R-410A"]
["Compressor","Type","","","","","تأرجح كتيم","تأرجح كتيم","تأرجح كتيم"]
["Dimensions","Unit","","العرض","mm","","658","855","855"]
["","","","العمق","mm","","289","328","328"]
["","","","الارتفاع","mm","","550","753","753"]
["الوزن","الوحدة","","","kg","","30","49","49"]
["Power supply","الطور","","","","","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240"]
["Notes","","","","","","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice.","(1) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة","(2) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","550"]
["","","","العرض","mm","658"]
["","","","العمق","mm","289"]
["الوزن","الوحدة","","","kg","28"]
["ضاغط","نوع","","","","تأرجح كتيم"]
["Operation range","Cooling","Ambient","Min.","درجة بمقياس الحوجلة الجافة","10"]
["","","","Max.","درجة بمقياس الحوجلة الجافة","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","18"]
["Sound pressure level","Cooling","","High","dBA","46"]
["سائل تبريد","النوع","","","","R-410A"]
["","السعة","","","kg","0.74"]
["","السعة","","","tCO2Eq","1.5"]
["","GWP","","","","2087.5"]
["وحدة التزويد بالطاقة","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]