{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":12,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B","RXS25K2V1B (Archived)"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","47","","47","48","48","48"]
["","Cooling","","High","ديسيبل أمبير","46","","46","48","48","48"]
["Standard Accessories","وصلة (تصريف)","","","","1","","1"]
["","Installation manual","","","","1","1","1","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.1","","2.1","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","السعة","","","كغ","1.0","","1.0","1.2","1.3","1.7"]
["","النوع","","","","R-410A","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","منخفض جداً","دورة في الدقيقة","780","","780","780","790","670"]
["","","التدفئة","منخفض جداً","دورة في الدقيقة","740","","740","740","780","670"]
["Piping connections","Level difference","IU - OU","Max.","m","15","","15","15","15","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","765","","765","765","765","825"]
["","","","العمق","mm","285","","285","285","285","300"]
["","","","الارتفاع","mm","550","","550","550","550","735"]
["الوزن","الوحدة","","","كغ","34","","34","34","39","47"]
["Fan","Air flow rate","التدفئة","منخفض جداً","قدم مكعب في الدقيقة","","","","904","960","1,522"]
["","","التبريد","منخفض جداً","قدم مكعب في الدقيقة","","","","1,063","1,080","1,727"]
["Power supply","الطور","","","","1~","","1~","1~","1~","1~"]
["","Frequency","","","هرتز","50","","50","50","50","50"]
["","Voltage","","","V","220-240","","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - SL: The silent fan level of the air flow rate setting","","(4) - SL: The silent fan level of the air flow rate setting","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة","(4) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة","","(5) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","mm","","550","","","","","550"]
["","","","العرض","mm","","765","","","","","765"]
["","","","العمق","mm","","285","","","","","285"]
["الوزن","الوحدة","","","كغ","","34","","","","","34"]
["محرك المروحة","السرعة","التبريد","منخفض جداً","دورة في الدقيقة","","780","","","","","780"]
["","","التدفئة","منخفض جداً","دورة في الدقيقة","","740","","","","","740"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","","","","","-10"]
["","","","Max.","°CDB","","46","","","","","46"]
["","Heating","Ambient","Min.","°CWB","","-15","","","","","-15"]
["","","","Max.","°CWB","","18","","","","","18"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","46","","","","","46"]
["","Heating","","High","ديسيبل أمبير","","47","","","","","47"]
["سائل تبريد","النوع","","","","","R-410A","","","","","R-410A"]
["","السعة","","","كغ","","1.0","","","","","1.0"]
["","السعة","","","tCO2Eq","","2.1","","","","","2.1"]
["","GWP","","","","","2087.5","","","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","m","","20","","","","","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","","","","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","","15","","","","","15"]
["Standard Accessories","Joint (drain)","","","","","1","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","1~","","","","","1~"]
["Power supply","Frequency","","","هرتز","","50","","","","","50"]
["","Voltage","","","V","","220-240","","","","","220-240"]
["Standard Accessories","سدادة المصرف","","","","","","","1","1","1"]