{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-N / 2MXM-A9"]
[]
[]
[]
[]
["","","","","CTXM15N2V1B / CTXM15N2V1B / 2MXM40A2V1B9","CTXM15N2V1B / CTXM15N2V1B / 2MXM50A2V1B9"]
["Cooling capacity","Nom.","","kW","3.00","3.00"]
["Heating capacity","Nom.","","kW","3.50","4.00"]
["Nominal efficiency","Annual energy consumption","","kWh","302","310"]
["","COP","","","4.35","4.58"]
["","EER","","","4.97","4.84"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","122","119"]
["","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","3.00","3.00"]
["","SEER","","","8.66","8.81"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","908","971"]
["","Capacity","Pdesign","kW","3.00","3.30"]
["","Energy efficiency class","","","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.41","2.65"]
["","SCOP/A","","","4.62","4.76"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]