{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":10,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FCAHG71GVEB / RZAG71M7V1B","FCAHG100GVEB / RZAG100M7V1B","FCAHG140GVEB / RZAG100M7V1B","FCAHG71GVEB / FCAHG71GVEB / RZAG100M7V1B","FCAHG125GVEB / RZAG125M7V1B","FCAHG140GVEB / RZAG140M7V1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","12.1 (1)","13.4 (1)"]
["Space cooling","Annual energy consumption","","kWh/a","308","452","419","325","905","1,014"]
["","Capacity","Pdesign","kW","6.80","9.50","9.50","9.50","12.1","13.4"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","9.52","9.52","9.52","9.52","9.52"]
["","Annual energy consumption","","kWh/a","1,427","2,771","2,836","2,515","2,942","3,002"]
["Heating capacity","Nom.","","kW","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","13.5 (2)","15.5 (2)"]
["Space cooling","SEER","","","7.72","7.35","7.93","10.2","8.02","7.93"]
["","Energy efficiency class","","","A++","A++","A++","A+++"]
["Space heating (Average climate)","SCOP/A","","","4.61","4.81","4.70","5.30","4.53","4.44"]
["","Energy efficiency class","","","A++","A++","A++","A+++"]
["Notes","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]