{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / 2MXM-A"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM40A2V1B","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM40A2V1B","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM50A2V1B","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B","FDXM25F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B","FDXM35F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B","FTXP20M5V1B9 / FDXM25F3V1B9 / 2MXM50A2V1B","FTXP20M5V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B","FTXP20M5V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM68A2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","5.00","5.00","5.00","5.00","5.00","4.50","5.00","5.00"]
["Space cooling","SEER","","","6.28","6.16","6.21","6.24","6.51","6.41","6.40","6.65","6.54","6.49"]
["","Annual energy consumption","","kWh/a","223","228","282","281","269","273","274","237","268","270"]
["","Capacity","Pdesign","kW","4.00","4.00","5.00","5.00","5.00","5.00","5.00","4.50","5.00","5.00"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","4.20","4.20","4.20","4.20","4.20","4.10","4.20","4.20"]
["","SCOP/A","","","4.01","4.05","3.78","3.79","3.86","3.82","3.89","3.78","3.78","3.84"]
["","Energy efficiency class","","","A+","A+","A","A","A","A","A","A","A","A"]
["","Pdh Heating capacity at -10°","","kW","2.61","2.62","3.42","3.43","3.55","3.44","3.57","3.35","3.42","3.54"]
["","Annual energy consumption","","kWh/a","1,117","1,106","1,555","1,550","1,523","1,538","1,509","1,516","1,555","1,530"]
["Nominal efficiency","Annual energy consumption","","kWh","563","556","779","769","712","760","704","628","729","716"]
["","EER","","","3.55","3.60","3.21","3.25","3.51","3.29","3.55","3.58","3.43","3.49"]
["","COP","","","4.13","4.17","3.66","3.64","3.61","3.62","3.61","3.68","3.69","3.72"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","","","","","","","6.8"]
["Heating capacity","Nom.","","kW","","","","","","","","","","","8.60"]
["Nominal efficiency","EER","","","","","","","","","","","","","2.73"]
["","COP","","","","","","","","","","","","","3.01"]
["","Annual energy consumption","","kWh","","","","","","","","","","","1245"]
["Space cooling","Energy efficiency class","","","","","","","","","","","","","A"]
["","Capacity","Pdesign","kW","","","","","","","","","","","6.80"]
["","SEER","","","","","","","","","","","","","5.43"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","438"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","","","","A"]
["","Capacity","Pdesign","kW","","","","","","","","","","","3.60"]
["","SCOP/A","","","","","","","","","","","","","3.81"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","","","","","3.10"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","1323"]
["Energy Efficiency Range","","","","","","","","","","","","","","A+++ ~ D"]