{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":26,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 2MXM-M"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM20M2V1B / 2MXM40M2V1B","FTXM20M2V1B / FTXM25M2V1B / 2MXM40M2V1B","FTXM20M2V1B / FTXM35M2V1B / 2MXM40M2V1B","FTXM25M2V1B / FTXM25M2V1B / 2MXM40M2V1B","FTXM25M2V1B / FTXM35M2V1B / 2MXM40M2V1B","FTXM20M2V1B / FTXM20M2V1B / 2MXM40M3V1B","FTXM20M2V1B / FTXM25M2V1B / 2MXM40M3V1B","FTXM20M2V1B / FTXM35M2V1B / 2MXM40M3V1B","FTXM25M2V1B / FTXM25M2V1B / 2MXM40M3V1B","FTXM25M2V1B / FTXM35M2V1B / 2MXM40M3V1B","FTXM20M2V1B / FTXM20M2V1B / 2MXM50M2V1B","FTXM20M2V1B / FTXM25M2V1B / 2MXM50M2V1B","FTXM20M2V1B / FTXM35M2V1B / 2MXM50M2V1B","FTXM20M2V1B / FTXM42M2V1B / 2MXM50M2V1B","FTXM20M2V1B / FTXM50M2V1B / 2MXM50M2V1B","FTXM25M2V1B / FTXM25M2V1B / 2MXM50M2V1B","FTXM25M2V1B / FTXM35M2V1B / 2MXM50M2V1B","FTXM25M2V1B / FTXM42M2V1B / 2MXM50M2V1B","FTXM35M2V1B / FTXM35M2V1B / 2MXM50M2V1B","FTXM35M2V1B / FTXM42M2V1B / 2MXM50M2V1B","FTXM35M2V1B / FTXM50M2V1B / 2MXM50M2V1B","FTXM42M2V1B / FTXM42M2V1B / 2MXM50M2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00","","","","","","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["Space cooling","SEER","","","8.53","8.50","8.19","8.36","8.11","","","","","","8.71","8.67","8.54","8.54","8.51","8.53","8.56","8.57","8.57","8.60","8.52","8.56"]
["","Annual energy consumption","","kWh/a","165","165","171","168","173","","","","","","161","182","205","205","206","205","205","204","205","204","206","205"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00","","","","","","4.00","4.50","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["","Energy efficiency class","","","A+++","A+++","A++","A++","A++","","","","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","3.20","","","","","","4.00","4.10","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","4.64","4.60","4.60","4.60","4.61","","","","","","4.61","4.61","4.61","4.63","4.68","4.61","4.62","4.65","4.66","4.67","4.75","4.70"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","","","","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.6","2.7","2.8","2.7","2.8","","","","","","3.4","3.4","3.4","3.4","3.4","3.4","3.4","3.4","3.4","3.4","3.4","3.4"]
["","Annual energy consumption","","kWh/a","966","973","974","974","971","","","","","","1,214","1,244","1,275","1,268","1,255","1,275","1,272","1,265","1,262","1,258","1,238","1,251"]
["Nominal efficiency","Annual energy consumption","","kWh","486","481","477","479","472","","","","","","471","535","619","615","609","624","616","612","609","604","599","601"]
["","EER","","","4.12","4.16","4.20","4.18","4.24","","","","","","4.25","4.21","4.04","4.07","4.11","4.01","4.06","4.09","4.11","4.14","4.18","4.16"]
["","COP","","","4.28","4.32","4.41","4.37","4.46","","","","","","4.09","4.10","4.12","4.13","4.15","4.08","4.05","4.03","4.01","4.00","3.94","3.98"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","","","","","","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","","","","","","A","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","4.20","","","","","","","","","","","5.60"]
["Cooling capacity","Nom.","","kW","","","","","","4.0","4.0","4.0","4.0","4.0"]
["Heating capacity","Nom.","","kW","","","","","","4.20","4.20","4.20","4.20","4.20"]
["Nominal efficiency","EER","","","","","","","","4.12","4.16","4.20","4.18","4.24"]
["","COP","","","","","","","","4.28","4.32","4.41","4.37","4.46"]
["","Annual energy consumption","","kWh","","","","","","486","481","477","479","472"]
["","Energy labeling Directive","Cooling","","","","","","","A","A","A","A","A"]
["","","Heating","","","","","","","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","","","","","","A+++","A+++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","4.00","4.00","4.00","4.00","4.00"]
["","SEER","","","","","","","","8.53","8.50","8.19","8.36","8.11"]
["","Annual energy consumption","","kWh/a","","","","","","165","165","171","168","173"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","3.20","3.20","3.20","3.20","3.20"]
["","SCOP/A","","","","","","","","4.64","4.60","4.60","4.60","4.61"]
["","Pdh Heating capacity at -10°","","kW","","","","","","3","3","3","3","3"]
["","Annual energy consumption","","kWh/a","","","","","","966","973","974","974","971"]
["Energy Efficiency Range","","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used."]
["","","","","","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Heating capacity","Min.","","kW","","","","","","","","","","","5.20","5.60","5.60","5.60","5.60","","5.60","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","","","","","","","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]