{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":12,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / RXM-N9"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / RXM20N2V1B9","FTXM20N2V1B / RXM20N5V1B9","FTXM25N2V1B / RXM25N2V1B9","FTXM25N2V1B / RXM25N5V1B9","FTXM35N2V1B / RXM35N5V1B9","FTXM35N2V1B / RXM35N2V1B9","FTXM42N2V1B / RXM42N2V1B9","FTXM50N2V1B / RXM50N2V1B9"]
["Outdoor unit","","","","RXM20N2V1B9","RXM20N5V1B9","RXM25N2V1B9","RXM25N5V1B9","RXM35N5V1B9","RXM35N2V1B9","RXM42N2V1B9","RXM50N2V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.30","1.30","1.40","1.40","","1.70"]
["","Nom.","","kW","2.00","2.00","2.50","2.50","3.40","3.40","","5.00"]
["","Max.","","kW","2.60","2.60","3.20","3.20","4.00","4.00","","6.00"]
["Heating capacity","Min.","","kW","1.30","1.30","1.30","1.30","1.40","1.40","","1.70"]
["","Nom.","","kW","2.50","2.50","2.80","2.80","4.00","4.00","","5.80"]
["","Max.","","kW","3.50","3.50","4.70","4.70","5.20","5.20","","7.70"]
["Nominal efficiency","Annual energy consumption","","kWh","219","219","278","278","402","402","","679"]
["","COP","","","5.00","5.00","5.00","5.00","4.04","4.04","","4.00"]
["","EER","","","4.57","4.57","4.50","4.50","4.23","4.23","","3.68"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","","A"]
["","","Heating","","A","A","A","A","A","A","","A"]
["Space cooling","Annual energy consumption","","kWh/a","81","81","101","101","138","138","","236"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","","A++"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","2.50","3.40","3.40","","5.00"]
["","SEER","","","8.65","8.65","8.65","8.65","8.65","8.65","","7.41"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","632","632","659","659","687","687","","1,369"]
["","Capacity","Pdesign","kW","2.30","2.30","2.40","2.40","2.50","2.50","","4.60"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","","A++"]
["","Pdh Heating capacity at -10°","","kW","2.24","2.24","2.30","2.30","2.35","2.35","","4.09"]
["","SCOP/A","","","5.10","5.10","5.10","5.10","5.10","5.10","","4.71"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Min.","","kW","","","","","","","1.70"]
["","Nom.","","kW","","","","","","","4.20"]
["","Max.","","kW","","","","","","","5.00"]
["Heating capacity","Min.","","kW","","","","","","","1.70"]
["","Nom.","","kW","","","","","","","5.40"]
["","Max.","","kW","","","","","","","6.00"]
["Nominal efficiency","EER","","","","","","","","","4.33"]
["","COP","","","","","","","","","4.12"]
["","Annual energy consumption","","kWh","","","","","","","485"]
["","Energy labeling Directive","Cooling","","","","","","","","A"]
["","","Heating","","","","","","","","A"]
["Space cooling","Energy efficiency class","","","","","","","","","A++"]
["","Capacity","Pdesign","kW","","","","","","","4.20"]
["","SEER","","","","","","","","","7.85"]
["","Annual energy consumption","","kWh/a","","","","","","","187"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","A++"]
["","Capacity","Pdesign","kW","","","","","","","4.00"]
["","SCOP/A","","","","","","","","","4.71"]
["","Pdh Heating capacity at -10°","","kW","","","","","","","3.67"]
["","Annual energy consumption","","kWh/a","","","","","","","1189"]
["Energy Efficiency Range","","","","","","","","","","A+++ ~ D"]