{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZASG100M7V1B","FUA125AVEB9 / RZASG125M7V1B","FUA71AVEB / RZASG71M2V1B","FUA71AVEB9 / RZASG71M2V1B"]
["Cooling capacity","Nom.","","kW","","","6.80 (1)","6.80 (1)"]
["Space cooling","SEER","","","","","6.16","6.16"]
["","Annual energy consumption","","kWh/a","","","386","386"]
["","Capacity","Pdesign","kW","","","6.80","6.80"]
["","Energy efficiency class","","","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","4.50","4.50"]
["","SCOP/A","","","","","3.90","3.90"]
["","Energy efficiency class","","","","","A","A"]
["","Annual energy consumption","","kWh/a","","","1,615","1,615"]
["Heating capacity","Nom.","","kW","","","7.50 (2)","7.50 (2)"]
["Cooling capacity","Nom.","","kW","9.5","12.1"]
["Heating capacity","Nom.","","kW","10.8","13.5"]
["Space cooling","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","9.5","12.1"]
["","SEER","","","5.83","5.49"]
["","Annual energy consumption","","kWh/a","570","1322"]
["Space heating (Average climate)","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","6","6"]
["","SCOP/A","","","4.01","3.84"]
["","Annual energy consumption","","kWh/a","2095","2188"]
["Notes","","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]