{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Space cooling","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Annual energy consumption","","kWh/a","","","","","","","","","371","371","371","371"]
["","Capacity","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Energy efficiency class","","","","","","","","","","","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Energy efficiency class","","","","","","","","","","","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Nominal efficiency","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["Notes","","","","","","","","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","","","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Nominal efficiency","Annual energy consumption","","kWh","","","","","","","","","","","835","835"]
["","COP","","","","","","","","","","","","","4.08","4.08"]
["","Energy labeling Directive","Cooling","","","","","","","","","","","","A","A"]
["","","Heating","","","","","","","","","","","","A","A"]
["Heating capacity","Nom.","","kW","","","","","","","","","","","7.50","7.50"]
["Notes","","","","","","","","","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]