{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":15,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UAT-AY1"]
[]
[]
[]
[]
["","","","","","UAT180AMY1","UAT240AMY1","UAT280AMY1","UAT320AMY1","UAT450AMY1","UAT560AMY1","UAT700AMY1","UAT850AMY1","UATC10AMY1","UATC12AMY1"]
["Sound pressure level","Cooling","","","dBA","63 (1)","65 (1)","66 (1)","68 (1)","","","","","80 (1)","80 (1)"]
["Evaporator piping connections","Condensation drain size","","OD","mm","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4","25.4"]
["Cooling capacity","Nom.","","","kW","","","","","43.961 (1)","58.614 (1)","73.268 (1)","87.921 (1)"]
["","Min.","","","kW","17.290","23.450","29.300","34.000","","","","","96.420","118.410"]
["Power input","Cooling","","Nom.","kW","5.61 (1)","8.10 (1)","9.98 (1)","11.56 (1)","15.60 (1)","20.70 (1)","27.56 (1)","35.96 (1)","39.87 (1)","46.80 (1)"]
["Sound power level","Cooling","","","dBA","","","","","70","70","74","74"]
["Dimensions","Unit","","Width","mm","1,100","1,300","1,300","1,300","1,990","1,990","2,250","2,250","2,252","2,252"]
["","","","Depth","mm","1,530","1,530","1,530","1,530","1,670","1,670","2,800","2,800","3,180","3,180"]
["","","","Height","mm","1,000","1,000","1,000","1,000","1,200","1,200","1,735","1,735","1,974","1,974"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey"]
["Weight","Unit","","","kg","","","","","665","765","1,200","1,350"]
["EER","","","","","3.08 (1)","2.89 (1)","2.94 (1)","2.94 (1)","2.82 (1)","2.83 (1)","2.66 (1)","2.44 (1)","2.42 (1)","2.53 (1)"]
["Condenser","Refrigerant","","Type","","R-22","R-22","R-22","R-22","R-22","R-22","R-22","R-22","R-22","R-22"]
["Evaporator","Supply side","Fan","Nominal ESP","Pa","100","100","100","100","196 (0.000)","196 (0.000)","294 (0.000)","294 (0.000)","300","300"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Name","","","","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151.","(2) - All units are being tested and comply to ISO5151."]
["","","","","","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit.","(4) - Sound pressure levels are according to JIS B 8615 standard. Position of the measurement is 1m in front and 1m below the unit."]
["","","","","","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle.","(5) - Designation based on cooling cycle."]